**BMP L612 – Sheet Flow Dispersion for Minimum Requirement #5 – The List Approach**

# Sheet flow dispersion BMPs shall be designed in accordance with the SWMM and Green Stormwater Infrastructure Typical Detail Figure 008 – Sheet Flow Dispersion for Driveways. A flowpath width of 10 feet is required for up to 20 feet of paved or impervious surface area. An additional 10 feet of flowpath is required for each additional 20 feet of impervious surface width or fraction thereof.

# Hard Surface Area Requiring Mitigation: Click here to enter text.

# Width of Paved Surface Discharging into Sheet Flow Dispersion BMP: Click here to enter text.

# Width of Vegetated Flowpath: Click here to enter text.