|  |
| --- |
| City of Tacoma Stormwater Management Manual – Infeasibility ChecklistSurface Type: Lawn and Landscaped AreasBMP L613: Post Construction Soil Quality and DepthVersion: 07/01/2021 |
| It is not necessary to answer all questions when determining if a BMP is feasible for Minimum Requirement #5 – The List Approach. Unless otherwise noted, a single answer of No means the BMP is considered infeasible for meeting Minimum Requirement #5 – The List Approach. Applicant may choose which questions to answer when determining feasibility.  |
| Questions #1-2 relate to infeasibility criteria that are based onconditions such as topography and distances to predetermined boundaries and certain design criteria.  |
| **Question Number** | **Question** | **Yes** | **No** | **NA** |
| 1 | Can the soil amendments be placed on slopes less than 33%? |[ ] [ ] [ ]
| 2 | Will installing sheet flow dispersion cause conflicts with any of the following? (An answer of yes means this BMP is infeasible.) Place a checkmark next to the applicable item (2a-2e). |[ ] [ ] [ ]
| 2a | Requirements of the Historic Preservation Laws and Archeology Laws, Federal Superfund or Washington State Model Toxics Control Act, Federal Aviation Administration requirements for airports, or Americans with Disability Act |[ ]
| 2b | Special zoning district design criteria adopted and being implemented through any City of Tacoma planning efforts |[ ]
| 2c | Public health and safety standards |[ ]
| 2d | Transportation regulations to maintain the option for future expansion or multi-modal use of public rights-of-way |[ ]
| 2e | Critical Area Preservation Ordinance  |[ ]