**BMP L603.b – Downspout Dispersion – Splashblocks Sizing for Minimum Requirement #5 – The List Approach**

# Splashblocks shall be designed in accordance with the SWMM and Green Stormwater Infrastructure Typical Detail Figure 006 – Splash Block. A maximum of 700 ft2 of roof area can drain to a single splashblock.

# Roof Area Requiring Mitigation: Click here to enter text.

# Roof Area Discharging to Splashblock: Click here to enter text.